Rockchip models Update Instructions

**(MK802IIIIS,MK802IV,MK902,V5,MK902II,MK68)**

Pls download img file and update tool from Rikomagic website: [www.rikomagic.com](http://www.rikomagic.com)


Tool: FactoryTool\_v1.39

Driver: DriverAssitant\_v4.4


1.Driver installation

Click the folder“DriverAssitant\_v4.4”，and click“DriverInstall.exe”You will get below picture：

Press”驱动安装”





After Installation success, click ”确定” to exist.




1. Find the“FactoryTool.exe”from FactoryTool\_V1.39, double click.

A. Load the Img file


Click“Firmware”button



Wait for 5-10 seconds, after the img file loaded, select“Restore”，then click“Run”。



Now the orange button changes to green.



B. Press the recover button, then connect **USB OTG or Slave** of the box with the computer via an USB cable. After 3-5 seconds, loose the recovery button.

**MK68 recovery button:**



**MK902II/MK902 recovery button:**





**V5 recovery button:**



**MK802IIIS,MK802IV recover button:**



3. You will get below picture.



This process needs 1-2 mins. After update successfully, you will get below picture.

